Here is the First Video, in Reheading the Dayan Pudi.
A) Making Kundal
1) Take 2 meters of Tasma.
2) Make a slit on one end of the tasma.
3) Pass the other end of the tasma through the slit to make a round
circle little bigger than the round Kundal Holder of the Dayan shell.
4) Pass it through the slit two or three more times and make it tight.
5) Now tie the Knot and as shown in the Video.
6) Cut the extra Tasma.
http://www.sohumentr.com/tabla/videos/making_kundal.wmv

Preparing the Shell and the Pudi for Reheading.
1) Sharp outer edge of the shell can make things difficult for
reheading hence its important to file the edge and make it little
round and smooth.
2) Apply bee wax on the outer edge and little below where the Gajra is
placed.
3) Use your thumb and evenly rub the wax on the edge.
4) Take the Pudi(up side down) in your left hand, dip your (right
hand)fingers in water and moisten the Bharti. Make sure that you dont
spill water on the area where the syahi is located.
5)Take a fine grain polish paper, Hold your fingers under the syahi,
and gently rub the maidan and syahi region. It helps in opening the
sound of the pudi. ( 5th step can be done before the 4th).
http://www.sohumentr.com/tabla/videos/Prp_shellRdhd.wmv

Video 3: Tying the Pudi to the shell with the kundal.
1) Fix the Pudi tight to the shell.
2) Tie one end of the rope to the kundal
3) Wind one loop around the shell and take the rope out from under the
Kundal. that will fix the kundal at the center.
4)start winding around the Shell as shown in the Video.
http://www.sohumentr.com/tabla/videos/Tying_rope.wmv

This Video explains how to Insert the Tasma through Pudis.
Knowing the Tasma. Which is outer side and which is inner side.
Image shows which side of the tasma should face outside while
inserting it in the pudi holes.
http://img177.imageshack.us/img177/8686/understandingvadiaj5.jpg

1) Insert a Screw Driver in the first hole so that it help slide the
tasma easily .

2) take around 3 meters tasma in the beginning and do as instructed in
the Video.
Video 4a:
http://www.sohumentr.com/tabla/videos/inserting_tasma1.wmv

3) After inserting into 4 to 5 holes, Pull all the Vadi and tie a knot
to the kundal(below the first end) as shown in the video.
Video 4b:
http://www.sohumentr.com/tabla/videos/inserting_tasma2.wmv

4) once all the 16 insertions are complete, tie the other end to the
kundal as shown in the video.
Video 4c:
http://www.sohumentr.com/tabla/videos/inserting_tasma3.wmv

Video Explains How to Pull the Tasma for the first time.
http://www.sohumentr.com/tabla/videos/first_timepull.wmv

Video explains how to Fix the Gatthas in the 1 Vadi, then 2 vadi and
then 3.
http://www.sohumentr.com/tabla/videos/insertingGattas.wmv

Video Explains how to Break syahi using Lavastone and Tune the Dayan
http://www.sohumentr.com/tabla/videos/brksyhi_tuning.wmv